Usage: bed2bed_display [options] [-a <min BED score>] [-b <max BED score>] [<] <BED file|stdin>
      - version 1.6.0
      where options are:
  		 -d|--debug                Produce Debug information
  		 -h|--help                 Show this Help text
  		 -f|--feature <ft>         Set Feature name <ft>
  		 -o|--oformat <1|2>        Set output Format (1:BED[Def] 2:BedGraph)
  		 --name <name>             Set name for track name field [def. name=SGA-feature]
  		 --desc <desc>             Set track description field [def. desc="ChIP-Seq Custom data"]
  		 --color <col>             Define the track color in comma-separated RGB values [def. 100,100,100]
  		 --autoscale  <on|off>     Data viewing paramenter: set auto-scale to UCSC data view [def=OFF]
  		 --always0    <on|off>     Data viewing paramenter: always include zero [def=OFF]
  		 --wfunction  <func>       Data viewing paramenter: windowing function [def=mean+whiskers|maximum|mean|minimum]
  		 --smoothing  <grade>      Data viewing paramenter: smoothing window [def=OFF[0], <grade>=0,2..16]
  		 --visibility <mode>       Display mode: [def=dense|full|hide] or [def=1|2|3]

	Convert BED file to BED format suitable for displaying ChIP-seq peaks.
 	Two formats are supported: 1) BED Track with Score field; 2) BedGraph.
 	For BED track format, only the graphical parameter 'visibility' can be set.

